For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Control Cable Adjusting Locknut | 23 N·m | 17 lb ft
Air Cleaner Assembly Bolts | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 9 N·m | 78 lb in
Camshaft Position (CMP) Sensor Housing Bolts | 15 N·m | 11 lb ft
Crankshaft Position (CKP) Sensor Bolt | 6 N·m | 54 lb in
ECT Sensor | 15 N·m | 11 lb ft
EGR Valve Pipe Bolts | 15 N·m | 11 lb ft
EGR Valve Pipe Midway Bolt | 10 N·m | 88 lb in
EGR Valve Bolts | 25 N·m | 18 lb ft
EVAP Canister Purge Valve Bracket Bolt | 11 N·m | 97 lb in
EVAP Canister Vent Solenoid Bracket Bolt | 11 N·m | 97 lb in
EVAP Tank Pressure Control Solenoid Valve Bracket Bolt | 25 N·m | 18 lb ft
Fuel Cut-Off Valve Screws | 1.6 N·m | 15 lb in
Fuel Filter Bracket Bolt | 11 N·m | 97 lb in
Fuel Filter Bracket-to-Fuel Filter Bolt | 11 N·m | 97 lb in
Fuel Pipe Guard Nuts | 15 N·m | 11 lb ft
Fuel Pressure Regulator Bolts | 10 N·m | 89 lb in
Fuel Rail Bolts | 23 N·m | 17 lb ft
Fuel Rail Plug Bolt | 30 N·m | 22 lb ft
Fuel Sender (fuel pump) Assembly Bolts | 5 N·m | 45 lb in
Fuel Tank Pressure Sensor Bolts | 1.6 N·m | 15 lb in
Fuel Tank Shield (Protector) Bolts | 50 N·m | 36 lb ft
Fuel Tank Straps Bolts | 50 N·m | 36 lb ft
HO2S 1 | 45 N·m | 32 lb ft
HO2S 2 | 45 N·m | 32 lb ft
IAC Valve Screws | 3.5 N·m | 30 lb in
Ignition Coil Bolts | 10 N·m | 89 lb in
MAP Sensor Screws | 3.5 N·m | 30 lb in
Negative Battery Cable-to-Negative Battery Terminal Retainer | 8 N·m | 72 lb in
PCM Bracket Bolts | 6 N·m | 54 lb in
PSP Switch | 27 N·m | 20 lb ft
Spark Plugs | 25 N·m | 18 lb ft
Throttle Body Bolts and Nuts | 25 N·m | 18 lb ft
TP Sensor Bolts | 3.5 N·m | 30 lb in
Vehicle Speed Sensor (A/T) Bolt | 6 N·m | 54 lb in