For 1990-2009 cars

### Removal Procedure

1. Disconnect the windshield washer pump electrical connector (3).
2. Remove the 3 bolts (2) which secure the washer solvent container (1).
3. Drain the washer solvent from the washer solvent container (1) into a clean drain pan (2).
4. Remove the windshield washer nozzle hose (5) from the windshield washer pump (1).
5. Remove the windshield washer pump (1) from the washer solvent container (3).

### Installation Procedure

1. Install the windshield washer pump (1) to the washer solvent container (3).
2. Install the windshield washer nozzle hose (5) to the windshield washer pump (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the washer solvent container (1) to the vehicle. Secure the container with 3 bolts (2).

Tighten
Tighten the washer solvent container bolts to 13 N·m (115 lb in).

4. Connect the windshield washer pump electrical connector (3).
5. Refill the washer solvent container with washer solvent, as necessary.