For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges, and Console.
2. Push up with a pick from behind the instrument panel in order to disengage the retaining tab on the bottom of the CRUISE CTRL/ OFF switch.
3. Slide the CRUISE CTRL/OFF switch out from the instrument panel.
4. Disconnect the CRUISE CTRL/OFF switch electrical connector.
5. Remove the CRUISE CTRL/OFF switch from the vehicle.

### Installation Procedure

1. Connect the electrical connector to the CRUISE CTRL/OFF switch.
2. Install the CRUISE CTRL/OFF switch to the instrument panel. Ensure that the retaining tabs are fully engaged.
3. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges, and Console.