For 1990-2009 cars

## Evaporative Emission Canister Replacement w/o ORVR

### Removal Procedure

1. Release the 4 retaining clips (2) on the air cleaner cover .
2. Disconnect the EVAP system vent hose from the air cleaner cover.
3. Lift the air cleaner cover and swing the cover away from the EVAP canister.
4. Disconnect the 3 EVAP hoses (1) from the EVAP canister.
5. Remove the EVAP canister (2) from the canister bracket in the engine compartment.
6. Inspect the EVAP purge system for carbon particle contamination before replacing the EVAP canister. Refer to Evaporative Emission System Cleaning .

### Installation Procedure

1. Install the EVAP canister (2) to the canister bracket in the engine compartment.
2. Connect the 3 EVAP hoses (1) to the EVAP canister.
3. Install the air cleaner cover onto the air cleaner assembly.
4. Close the 4 retaining clips (2) on the air cleaner cover .
5. Connect the EVAP system vent hose to the air cleaner cover.

## Evaporative Emission Canister Replacement with ORVR

### Removal Procedure

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

Notice: The EVAP canister may have released carbon particles which caused this part to fail and may cause damage to other components. Check the EVAP canister for loose carbon before returning the vehicle to service.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the vapor hose (1) from the EVAP canister (2) by squeezing the connector as shown.
3. Disconnect the two hoses (1) from the EVAP canister (2).
4. Disconnect the electrical connector of the EVAP canister vent solenoid.
5. Remove the four fasteners and the EVAP canister bracket from the vehicle chassis.
6. Remove the EVAP canister from the bracket.

### Installation Procedure

1. Install the EVAP canister to the bracket.

Install the canister and bracket to the vehicle chassis.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the canister and bracket to the vehicle with the four fasteners.

Tighten
Tighten the fasteners to 10 N·m (89 lb in).

3. Connect the three hoses (1) to the EVAP canister (2).
4. Connect the electrical connector of the EVAP canister vent solenoid.
5. Lower the vehicle.