For 1990-2009 cars

### Removal Procedure

1. Remove the front speaker grill (1) from the instrument panel by pulling the grill straight out with a flat-bladed screwdriver.
2. Remove the front speaker screw (3).
3. Remove the front speaker (5) from the instrument panel (4).
4. Disconnect the speaker electrical connector.
5. Remove the front speaker (5) from the vehicle.

### Installation Procedure

1. Connect the speaker electrical connector.
2. Install the front speaker (5) to the vehicle. Secure the front speaker (5) to the instrument panel (4) with 1 screw (3).
3. Install the front speaker grill (1) to the instrument panel (4).