For 1990-2009 cars

### Removal Procedure

1. Disengage the 14 plastic retaining clips on the rear door inner trim panel. Remove the rear door inner trim panel.
2. Remove the 3 screws (4) which secure the rear wiper motor (3) to the rear door.
3. Remove the screw which secures the wiper motor ground wire (1) to the rear door.
4. Remove the rear wiper motor ground wire (1) from the rear door.

Important: Do not service the rear wiper motor crank arm separately. Do not disconnect the motor crank arm from the rear wiper motor. The crank arm is positioned on the wiper motor in order to allow the rear wiper arm to return to the arms normal park position.

5. Gently pry the rear wiper linkage from the rear wiper motor crank arm.
6. Remove the rear wiper motor from the vehicle.

### Installation Procedure

1. Install the rear wiper motor to the rear door.
2. Install the rear wiper linkage to the rear wiper motor crank arm.
3. Install the 3 screws (4) which secure the rear wiper motor (3) to the rear door.
4. Connect the rear wiper motor ground wire (1) to the rear door. Secure the rear wiper motor ground wire with 1 screw.
5. Install the rear door inner trim panel. Secure the rear door inner trim panel with 14 plastic retaining clips.