For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster assembly from the instrument panel. Refer to Instrument Cluster Replacement .
3. Remove the instrument cluster lens and bezel assembly from the instrument cluster housing by releasing the 8 black plastic tabs in order to gain access to the temperature gauge (9).
4. Remove the 3 screws (4) and the temperature gauge from the instrument cluster housing.

### Installation Procedure

1. Install the temperature gauge to the instrument cluster housing. Secure the gauge with the 3 screws (4).
2. Install the instrument cluster lens and the bezel to the instrument cluster housing.
3. Install the instrument cluster assembly to the instrument panel. Refer to Instrument Cluster Replacement .
4. Connect the negative battery cable.