For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear coil spring (2). Refer to Coil Spring Replacement .
3. Remove the spring bump stop (1).

### Installation Procedure

1. Install the spring bump stop (1) to the vehicle.
2. Install the rear coil spring (2). Refer to Coil Spring Replacement .
3. Lower the vehicle.