For 1990-2009 cars

1. Rotate the transmission to the fluid pan side.
2. Remove the following fluid pan components:

• | The 14 bolts

• | The fluid pan (2)

• | The gasket

3. Remove the four fluid pipes in the following order:

3.1. | The brake applying

3.2. | The reverse brake

3.3. | The lube applying

3.4. | The forward clutch

4. Unclip the TCC solenoid (3) and shift solenoid wiring harness from the fluid filter screen (2).
5. Remove the six fluid filter screen bolts (1) from the valve body.
6. Inspect the fluid filter screen mesh for the following particulate matter:

• | Clutch material

• | Steel particles