For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check
2 | Use a J 35616-200 unpowered test lamp in order to backprobe the left rear power window switch connector from cavity 1 to ground. Does the test lamp light? | -- | Go to Step 4 | Go to Step 3
3 | Repair the open in the BLU or the BLU/WHT wire between the left rear power window switch and SP370. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
4 | Replace the left rear power window switch. Refer to Rear Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --