For 1990-2009 cars

### Removal Procedure

1. Remove the front seat cushion. Refer to Front Seat Cushion Replacement .
2. Release the J-retainers which secure the seat cushion cover (1) to the seat cushion.
3. Remove the seat cushion cover (1) from the seat cushion.

### Installation Procedure

1. Install the seat cushion cover (1) to the seat cushion. Secure the cover with the J-retainers.
2. Install the front seat cushion. Refer to Front Seat Cushion Replacement .