For 1990-2009 cars

### Shock Absorber Inspection

• | Inspect the shock absorber for deformation or damage.

• | Inspect the bushings for wear or damage.

• | Inspect the shock absorber for evidence of oil leakage.

Replace any defective part.

### Lower Control Arm, Upper Control Arm, Rear Axle Tie Rod Inspection

• | Inspect the lower control arm (5) for cracks, deformation, or damage.

• | Inspect the upper control arm (3) for cracks, deformation, or damage.

• | Inspect the rear axle tie rod (4) for cracks, deformation, or damage.

• | Inspect the bushings for wear and damage.

Replace any defective part.

### Axle Housing and Coil Spring Inspection

• | Inspect the coil spring (1) for cracks, deformation, or damage.

• | Inspect the axle housing (2) for evidence of oil leakage.

Replace any defective part.

#### Rear Suspension Fasteners

Inspect for tightness each bolt and nut used for fastening suspension parts. Tighten loose fasteners to the specified torque. Refer to Fastener Tightening Specifications .

### Bearing Retainer and Axle Shaft Inner Oil Seal Inspection

• | Inspect the backside of the brake backing plate (1) for oil leakage. If you find any leakage, replace the defective oil seal.

• | Inspect the oil seal lip (1). If you find any oil leakage or a worn lip, replace the defective oil seal.

• | Inspect inside of the brake drum for grease or oil leakage.