For 1990-2009 cars

### Removal Procedure

1. Remove the 14 plastic retaining clips from the rear door interior trim panel (1).
2. Remove the rear door interior trim panel (1).
3. Pull the water deflector away from the rear door.
4. Inspect the water deflector for tears and holes.
5. Repair the water deflector, as needed, using waterproof tape on either side of the deflector.

### Installation Procedure

1. Apply adhesive to the back of the water deflector.
2. Install the water deflector to the door.
3. Install the rear door interior trim panel (1) to the rear door (2). Secure the trim panel with the 14 retaining clips.