For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: When the pedal assembly is pressed to the floor, the shift lever does not move freely in and out of reverse gear.
1 | Check for any obstruction in the movement of the clutch pedal. Was there any obstruction found? | Go to Step 2 | Go to Step 3
2 | Remove the obstruction. Does the clutch work properly? | System OK | Go to Step 3
3 | Check the clutch pedal mechanism. Refer to Clutch Pedal Replacement . Does the clutch work properly? | System OK | Go to Step 4
4 | Check for air in the hydraulic clutch system. Is there air in the hydraulic clutch system? | Go to Step 5 | Go to Step 6
5 | Bleed the hydraulic clutch system. Refer to Hydraulic Clutch Bleeding . Does the clutch work properly? | System OK | Go to Step 6
6 | Check the master cylinder for worn seals. Are the seals worn? | Go to Step 7 | Go to Step 8
7 | Replace the necessary components. Refer to Clutch Master Cylinder Replacement . Does the clutch work properly? | System OK | Go to Step 8
8 | Check for a worn or damaged actuator cylinder. Is the actuator cylinder worn or damaged? | Go to Step 9 | Go to Step 10
9 | Replace the actuator cylinder. Refer to Clutch Actuator Cylinder Replacement . Does the clutch work properly? | System OK | Go to Step 10
10 | Inspect the clutch assembly for the following:

• | Damaged or worn clutch pressure plate

• | Binding clutch disc

Are the clutch components OK?

--

Go to Step 11

11 | Replace the clutch assembly. Refer to Clutch Assembly Replacement . Does the clutch work properly? | System OK | --