For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: The clutch release bearing is noisy with the clutch fully engaged or during engagement.
1 | Inspect the clutch release bearing. Is the clutch release bearing worn? | Go to Step 2 | Go to Step 3
2 | Replace the clutch release bearing. Refer to Release Bearing Replacement . Is the clutch release bearing still noisy? | -- | System OK
3 | Check the clutch release bearing for binding on the transmission bearing retainer. Is the release bearing binding on the transmission bearing retainer? | Go to Step 4 | --
4 | Clean and lubricate the affected area. Is the release bearing sliding surface on the input shaft contaminated? | System OK | --