For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the system Descriptions and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Verify the vehicle leans or sways in corners. Does the vehicle lean or sway in corners? | Go to Step 3 | System OK
3 | Inspect the springs for wear or damage. Are the springs worn or damaged? | Go to Step 6 | Go to Step 4
4 | Inspect the front stabilizer shaft, the links, the insulators, and the brackets for wear or damage. Are any front stabilizer shaft components worn or damaged? | Go to Step 7 | Go to Step 5
5 | Inspect the rear axle tie rod and the rear suspension control arms for wear or damage. Are any rear suspension components worn or damaged? | Go to Step 8 | Go to Step 2
6 | Replace the springs. Refer to Front Coil Springs Replacement in Front Suspension or to Coil Spring Replacement in Rear Suspension. Did you complete the repair? | Go to Step 9 | --
7 | Replace the front stabilizer shaft components as necessary. Refer to the following procedures in Front Suspension:

• | Stabilizer Shaft Replacement

• | Stabilizer Shaft Link Replacement

• | Stabilizer Shaft Insulator Replacement

Did you complete the repair?

Go to Step 9

--

8 | Replace the rear suspension components as necessary. Refer the following procedures in Rear Suspension:

• | Tie Rod Replacement

• | Rear Axle Upper Control Arm Replacement

• | Rear Axle Lower Control Arm Replacement

Did you complete the repair?

Go to Step 9

--

9 | Operate the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2