For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Inspect the for the following conditions:

1. Proper battery installation.
2. Proper battery terminal installation.
3. Proper battery cable installation.
4. Clean and tight ground connections.
5. Excessive battery terminal corrosion.
6. Cracking or other damage.
7. Correct battery voltage.
8. The battery hydrometer for a green dot.
9. The generator wiring for damage or poor connections.
10. The generator mounting bolts for proper torque.
11. The generator drive belt for proper installation.

• | The battery is properly installed.

• | The battery terminals are properly installed.

• | The battery cables are properly installed.

• | The ground connections are clean and tight.

• | The battery terminals are clean and tight.

• | The battery is not physically damaged.

• | Battery voltage is approximate 11.5-13.0 volts.

• | The battery hydrometer displays a green dot.

• | the wiring is in serviceable condition.

• | Battery Hydrometer Displays Dark or Yellow Dot .

• | Battery Common Causes of Malfunction .

• | Battery Load Test .

• | Battery Charging .

• | Clean, tighten or repair the wiring and connections as necessary. Refer to Wiring Repairs in Wiring Systems.

• | Battery Not Operating Properly .

• | Battery Check .

• | Battery Terminal Check .

• | Battery Hydrometer Displays Yellow Dot .

• | Generator Replacement .

• | Drive Belt Replacement in Engine Mechanical.

2 | Turn the ignition switch to the key ON engine OFF position | The charge indicator lamp lights. | Charge Indicator Inoperative
3 | Start the engine | The charge indicator lamp goes out after the engine starts. | Charge Indicator Always On
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.