For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Raise and Support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Remove the vehicle speed sensor electrical connector.
4. If 2WD equipped, remove the 1 bolt (1) and the vehicle speed sensor (2) from the transmission.

### Installation Procedure

1. If 2WD equipped, install the 1 bolt (1) and the vehicle speed sensor (2) to the transmission.
2. Install the vehicle speed sensor electrical connector.
3. Lower the vehicle.
4. Connect the negative battery cable.