For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for loose system components (heat shields, hangers, etc.) Are any exhaust system components loose? | -- | Go to Step 2 | Go to Step 3
2 | Tighten any loose components. Does the exhaust system vibrate or rattle? | -- | Go to Step 3 | System OK
3 | Check for misaligned system components. Are any system components misaligned? | -- | Go to Step 4 | Go to Step 5
4 | Align any misaligned system components. Does the exhaust system vibrate or rattle? | -- | Go to Step 5 | System OK
5 | Check for bent or damaged support brackets or mounts. Are there any bent or damaged support brackets or mounts? | -- | Go to Step 6 | --
6 | Repair any bent or damaged support brackets or mounts. Does the exhaust system vibrate or rattle? | -- | -- | System OK