For 1990-2009 cars

### Removal Procedure

1. Remove the 4 screws and the knee bolster trim panel (2).
2. Gently pull the top portion of the knee bolster trim panel (2) in order to release the 2 clips.
3. Remove the 2 bolts and the knee bolster (1) from the instrument panel.

### Installation Procedure

1. Install the knee bolster (1) to the instrument panel. Secure the knee bolster with the 2 bolts.
2. Install the knee bolster trim panel (2). Secure the trim panel with the 2 clips and the 4 screws.