For 1990-2009 cars

### Removal Procedure

1. Remove the Front Wheel Hub. Refer to Front Wheel Hub, Bearing, and Seal Replacement or Front Wheel Hub, Bearing, and Seal Replacement in Front Suspension.
2. Remove the ABS reluctor ring (1) from the wheel hub (2) by prying the ring away from the hub.

### Installation Procedure

#### Tools Required

J 39245 ABS Sensor Ring Installer

1. Using J 39245 , press the ABS reluctor ring (2) onto the wheel hub.
2. Install the Front Wheel Hub. Refer to Front Wheel Hub, Bearing, and Seal Replacement or Front Wheel Hub, Bearing, and Seal Replacement in Front Suspension.
3. Perform Diagnostic System Check - ABS .