For 1990-2009 cars

### Removal Procedure

1. Discharge and recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the front grille. Refer to Grille Replacement in Exterior Trim.
3. Remove the air cleaner hose.
4. Slide the EVAP canister out of its bracket and position aside.
5. Remove the bolt (1) from the expansion valve.
6. Slide the plate (2) counterclockwise and remove the evaporator outlet tube from the expansion valve.
7. Disconnect the fitting from the compressor suction pipe (4).
8. Remove the 2 bolts from the evaporator outlet tube hold-down retainers.
9. Remove the evaporator outlet tube from the body mounted retainers.
10. Remove the evaporator outlet tube from the vehicle.

### Installation Procedure

1. Install new O-rings coated with mineral base 525 viscosity refrigerant oil.
2. Install the evaporator outlet tube to the vehicle.
3. Install the evaporator outlet tube to the body mounted retainers.
4. Install the evaporator outlet tube to the expansion valve.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Slide the plate (2) clockwise and install the bolt.

Tighten
Tighten the bolt (1) to 35 N·m (26 lb ft).

6. Connect the evaporator outlet tube to the compressor suction hose (4).

Tighten
Tighten the fitting to 35 N·m (26 lb ft).

7. Install the evaporator outlet tube hold-down retainers. Secure with the 2 bolts.
8. Install the EVAP canister to its bracket.
9. Install the air cleaner hose.
10. Install the front grille. Refer to Grille Replacement in Exterior Trim.
11. Evacuate and recharge the air conditioning system. Refer to Refrigerant Recovery and Recharging .
12. Operate the A/C system and test for refrigerant leaks. Refer to Leak Testing .