For 1990-2009 cars

### Removal Procedure

1. Remove the screw from the front seat belt trim bezel (3).
2. Remove the rear body side lower trim panel (1) from the vehicle, by disengaging the plastic retainers.

### Installation Procedure

1. Install the rear body side lower trim panel (1) to the vehicle. Ensure that the plastic retainers are fully engaged.
2. Install the front seat belt trim bezel (3) to the vehicle. Secure the bezel with the screw.