For 1990-2009 cars

### Removal Procedure

1. Mark the position of the rear side door lock striker (4) on the door jamb for ease of installation.
2. Remove 2 screws and the rear side door lock striker (4) from the door jamb.

### Installation Procedure

1. Install the rear side door lock striker (4) to the door jamb. Secure the striker with 2 screws.
2. Adjust the striker vertical measurement so that the striker (1) shaft aligns with the center of the door lock (2).
3. Adjust the lock striker (1)-to-door distance to 13-15 mm (0.51-0.59 in) by installing or removing shims (2) as necessary.
4. Keeping the lock striker (1) level, move the striker sideways in order to adjust door flushness with the quarter panel (3). Refer to Door Adjustment Specifications .