For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Definition: This table diagnoses a right rear window inoperative condition when using the remote right rear window switch located in the center console.
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check
2 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window motor connector from cavity 2 to ground.
2. Depress the right rear remote power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 3

Go to Step 7

3 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window motor connector from cavity 1 to ground.
2. Lift the right rear remote power window switch to the UP position.

Does the test lamp light?

--

Go to Step 4

Go to Step 16

4 |

1. Disconnect the right rear power window motor connector.
2. Connect a J 35616-200 unpowered test lamp from cavity 2 to B+.

Does the test lamp light?

--

Go to Step 5

Go to Step 21

5 | Connect a J 35616-200 unpowered test lamp from the right rear power window motor connector cavity 1 to B+. Does the test lamp light? | -- | Go to Step 6 | Go to Step 26
6 | Replace the right rear power window motor. Refer to Rear Side Door Window Regulator Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
7 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 5 to ground.
2. Depress the right rear remote power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 8

Go to Step 9

8 | Repair the open in the RED wire between the right rear power window switch and the right rear power window motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
9 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 2 to ground.
2. Depress the right rear remote power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 10

Go to Step 11

10 | Replace the right rear power window switch. Refer to Rear Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
11 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear remote power window switch connector from cavity 5 to ground.
2. Depress the right rear remote power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 12

Go to Step 13

12 | Repair the open in the RED/WHT or the RED/BLK wire between the right rear remote power window switch and the right rear power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
13 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear remote power window switch connector from cavity 1 to ground. Does the test lamp light? | -- | Go to Step 14 | Go to Step 15
14 | Replace the right rear remote power window switch. Is the repair complete? | -- | Go to Power Windows System Check | --
15 | Repair the open in the BLU/WHT wire between the right rear remote power window switch and SP370. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
16 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 3 to ground.
2. Lift the right rear remote power window switch to the UP position.

Does the test lamp light?

--

Go to Step 17

Go to Step 18

17 | Repair the open in the YEL wire between the right rear power window switch and the right rear power window motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
18 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 4 to ground.
2. Lift the right rear remote power window switch to the UP position.

Does the test lamp light?

--

Go to Step 10

Go to Step 19

19 |

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right rear remote power window switch connector from cavity 3 to ground.
2. Lift the right rear remote power window switch to the UP position.

Does the test lamp light?

--

Go to Step 20

Go to Step 13

20 | Repair the open in the GRN/WHT or the GRN/BLK wire between the right rear remote power window switch and the right rear power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
21 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 5 to B+. Does the test lamp light? | -- | Go to Step 8 | Go to Step 22
22 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 2 to B+. Does the test lamp light? | -- | Go to Step 10 | Go to Step 23
23 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear remote power window switch connector from cavity 5 to B+. Does the test lamp light? | -- | Go to Step 12 | Go to Step 24
24 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear remote power window switch connector from cavity 4 to B+. Does the test lamp light? | -- | Go to Step 14 | Go to Step 25
25 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 3 to B+. Does the test lamp light? | -- | Go to Step 17 | Go to Step 26
26 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear power window switch connector from cavity 4 to B+. Does the test lamp light? | -- | Go to Step 10 | Go to Step 27
27 | Use a J 35616-200 unpowered test lamp from the right rear remote power window switch connector from cavity 3 to B+. Does the test lamp light? | -- | Go to Step 20 | Go to Step 28
28 | Use a J 35616-200 unpowered test lamp in order to backprobe the right rear remote power window switch connector from cavity 2 to B+. Does the test lamp light? | -- | Go to Step 14 | Go to Step 29
29 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 5 to B+. Does the test lamp light? | -- | Go to Step 30 | Go to Step 31
30 | Repair the open in the BRN or the BRN/BLK wire between the left front power window/door lock switch and SP371 or in the BRN/BLK wire between SP371 and the left rear remote power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
31 | Replace the left front power window/door lock switch. Refer to Door Lock and Side Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --