For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn ignition switch to ON.
2. Position and press the rear Wiper switch to the ON position.

Rear wiper operates.

Rear Wiper Inoperative

2 | Press rear wiper switch to OFF. | Rear wiper stops in the park position. |

• | Rear Wiper Always On

• | Rear Wiper Blade Does Not Park

3 | Press and hold the rear washer switch. | Rear washer pump operates and rear wiper completes at least one full sweep. |

• | Rear Washer Inoperative

• | Rear Wiper Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.