For 1990-2009 cars

#### Front Seats

(1) | Right Front Seat Head Restraint Guides
(2) | Right Front Seat Back Cushion
(3) | Seat Cushion Pad and Frame
(4) | Right Front Seat Outer Adjuster Finish Cover
(5) | Right Front Seat Outer Adjuster
(6) | Seat Adjuster Handle
(7) | Right Front Seat Inner Adjuster
(8) | Seat Inner Adjuster Finish Cover
(9) | Left Front Seat Outer Adjuster
(10) | Left Front Seat Outer Adjuster Finish Cover
(11) | Left Front Seat Inner Adjuster
(12) | Seat Adjuster Lateral Rod
(13) | Left Front Seat Back Cushion
(14) | Left Front Seat Head Restraint Guides
(14) | Left Front Seat Head Restraint Guides
(15) | Front Seat Head Restraints

Caution: Do not try to change the designed seat position by changing the seat adjuster-to-floor pan anchor placement or the seat adjuster-to-seat frame anchor placement. Changing the designed seat position could affect the safe performance of the seat and cause personal injury.

The vehicle is equipped with low backed bucket seats with separate head restraints (15). The seat cushions and seat back cushions have formed foam pads which fit the contour of the seat cushion frame and the seat back cushion frame. The front seats are equipped with a seat adjuster handle (6) and a seat back adjuster. The seat adjuster handle (6) is located under the front of the seat cushion (3). Lift the seat adjuster handle (6) in order to move the seat forward and rearward. The seat back adjuster is an integral part of the outer seat adjuster (5 or 9). Lift the seat back recliner handle in order to raise and lower the seat back. The 2-door models are equipped with a knob on the lower portion of the passengers seat back. Push the knob down in order to fold the seat back forward and allow the passenger seat to be pushed forward. Slide the seat to a full rearward position and return the seat back to the upright position in order to lock the seat into place.