For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
3. Remove the boot (3). Refer to Steering Gear Boot Replacement - On Vehicle .
4. Unstake the lock washer (2).
5. Remove the inner tie rod (1) from the rack (3).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install a new lock washer (2) and inner tie rod (1) to the rack.

Tighten
Tighten the inner tie rod to 85 N·m (61.5 lb ft).

2. Stake the lock washer at the flat spots on the inner tie rod.
3. Install the boot (3). Refer to Steering Gear Boot Replacement - On Vehicle .
4. Install the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
5. Lower the vehicle.