For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the following components from the vehicle:

2.1. | The screw

2.2. | The 11 plastic retainers

2.3. | The front fender liner (1)

### Installation Procedure

1. Install the front fender liner (1) to the vehicle. Secure the liner with the 11 plastic retainers and 1 screw.
2. Lower the vehicle.