For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door check pin (2) and position the rear side door check (3) away from the door jamb.
2. Gently pry loose the plastic retainers which secure the rear side door weatherstrip (4) and remove the weatherstrip from the rear side door.

### Installation Procedure

1. Install the rear side door weatherstrip (4) to the rear side door. Ensure that the plastic retainers are fully engaged.
2. Install the rear side door check (3) to the door jamb. Secure the check with the pin (2).