For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the rear axle tie rod bolts (1,3), the nut, and the washers.
3. Remove the rear axle tie rod (2).

### Installation Procedure

Important: DO NOT tighten the bolts. The weight of the vehicle must be on the tires and wheels before tightening the bolts.

1. Install the following components to the rear axle and to the vehicle body:

• | The rear axle tie rod (2)

• | The 2 washers

• | The 2 bolts (1,3)

• | The nut

2. Lower the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. With the weight of the vehicle on the tires and wheels, tighten the bolts (1,3).

Tighten
Tighten the bolts to 90 N·m (65.0 lb ft).