For 1990-2009 cars

### Removal Procedure

1. Push both sides of the glove box in towards the center (3).
2. Pull the glove box down.
3. Disconnect the fuel pump relay electrical connector.
4. Remove the fuel pump relay (1) from the bracket.

### Installation Procedure

1. Install the fuel pump relay (1) to the bracket.
2. Connect the fuel pump relay electrical connector.
3. Push the glove box up and back into the closed position.