For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the hood.
2. Twist the park/turn lamp bulb socket counterclockwise and remove the socket from the headlamp assembly.
3. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Install the park/turn lamp bulb socket to the headlamp assembly and twist clockwise in order to secure the socket.
3. Lower the hood.