For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges, and Console.
2. Disconnect the power door lock module electrical connector.
3. Remove the power door lock module (1) assembly from the IP bracket.

### Installation Procedure

1. Install the power door lock module (1) to the IP bracket.
2. Connect the power door lock module electrical connector.
3. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges, and Console.