For 1990-2009 cars

### Removal Procedure

1. Remove the folding top side rail garnish moldings. Refer to Folding Top Side Rail Replacement .
2. Remove the following components from the vehicle:

2.1. | The 2 screws

2.2. | The folding top side body joint cover (1)

### Installation Procedure

1. Install the folding top side body joint cover (1) to the vehicle. Secure the cover with the 2 screws.
2. Install the folding top side rail garnish moldings. Refer to Folding Top Side Rail Replacement .