For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the following components from the vehicle:

• | The 10 plastic retainers

• | The rear wheelhouse panel liner (1)

### Installation Procedure

1. Install the rear wheelhouse panel liner (1) to the vehicle. Secure the liner with the 10 plastic retainers.
2. Lower the vehicle.