For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the hood.
2. Remove the 6 plastic retainers which secure the air inlet screen over the rear hood weatherstrip.
3. Remove the plastic retainer which secures each side of the weatherstrip.
4. Pull the rear hood weatherstrip from the cowl flange.

### Installation Procedure

1. Install the rear hood weatherstrip to the cowl flange by pressing into place. Secure the weatherstrip with the 8 plastic retainers.
2. Lower the hood.