For 1990-2009 cars

### Removal Procedure

1. Slide the rearview mirror trim bezel (1) off of the mirror (2).
2. Remove the two screws that secure the inside rearview mirror (2).
3. Remove the rearview mirror (2) from the vehicle.
4. Remove each screw that secures each sunshade support (1).
5. Remove the sunshade support (1).
6. Remove the 2 screws from each sunshade.
7. Remove both sunshades (2) from the vehicle.
8. Pull the dome lamp lens (1) off of the dome lamp (2).
9. Remove the 2 screws that secure the dome lamp (2) to the roof.
10. Lower the dome lamp from the roof.
11. Remove the screw and the dome lamp bracket.
12. Disconnect the dome lamp electrical connector.
13. Remove the dome lamp (2) from the vehicle.
14. Remove the 2 screws from each assist handle (3, 8).
15. Remove the assist handles (3, 8) from the vehicle.
16. Remove the screw from each coat hook and remove the coat hooks (2, 9) from the vehicle.
17. Loosen the front door opening finishing lace along both windshield side garnish moldings.
18. Gently pry both windshield side garnish moldings loose.
19. Remove the windshield side garnish moldings from the vehicle.
20. Gently pry the front headlining trim loose.
21. Remove the front headlining trim from the vehicle.
22. Remove the front and rear seat belt guide loop anchor bolts.
23. Loosen the rear door opening weatherstrip (1) along the rear quarter window interior trim and the headlining trim (2).
24. Remove the rear quarter window trim. Refer to Rear Quarter Upper Trim Panel Replacement .
25. Remove the 4 plastic retainers and the rear headlining trim from the vehicle.
26. Remove the 4 plastic retainers and the headlining (2) from the vehicle.

### Installation Procedure

1. Install the headlining (2) to the vehicle. Secure the headlining with the 4 plastic retainers.
2. Install the rear headlining trim to the vehicle. Secure the rear headlining trim with the 4 plastic retainers.
3. Install the rear quarter window trim. Refer to Rear Quarter Upper Trim Panel Replacement .
4. Press the rear door opening weatherstrip (1) into place.
5. Install the front and rear seat belt guide loop anchor bolts.

Tighten
Tighten the front and rear seat belt guide loop anchor bolts to 45 N·m (33 lb ft).

6. Install the front headlining trim to the vehicle. Press the front trim into place.
7. Install the windshield side garnish molding to the vehicle. Press the molding into place.
8. Press the front door opening finishing lace into place along both of the windshield side garnish moldings.
9. Install the coat hooks (2, 9) to the vehicle. Secure each hook with 1 screw.
10. Install the assist handles (3, 8) to the vehicle. Secure each handle with 2 screws.
11. Connect the dome lamp electrical connector.
12. Install the dome lamp bracket. Secure the bracket with the screw.
13. Install the dome lamp (6) to the roof. Secure the lamp with 2 screws.
14. Install the dome lamp lens (1) to the dome lamp (2).
15. Install the sunshades (2) to the vehicle. Secure each sunshade (2) with 2 screws.
16. Install the sunshade supports (1) to the vehicle. Secure each support (1) with 1 screw.
17. Install the inside rearview mirror (2) to the vehicle. Secure the mirror with 2 screws.
18. Slide the inside rearview mirror trim bezel (1) onto the mirror.