For 1990-2009 cars

### Removal Procedure

1. Remove the battery from the vehicle. Refer to Battery Replacement .
2. Remove the plastic liner.
3. Remove the wiring harness clip from the engine side of the battery tray.
4. Remove the 4 bolts from the battery tray.
5. Remove the battery tray from the vehicle.

### Installation Procedure

1. Install the battery tray into the vehicle.
2. Install the 4 bolts.
3. Install the wiring harness clip to the battery tray.
4. Install the plastic liner.
5. Install the battery into the vehicle. Refer to Battery Replacement .