For 1990-2009 cars

1. Remove the following manual lever components from the manual shaft:

• | The nut

• | The washer

• | The lever

2. Unstake the lock plate behind the manual shaft nut.
3. Remove the following components from the transmission range switch:

• | The manual shaft nut

• | The lock plate

4. Remove the transmission range switch retaining bolt.
5. Remove the transmission range switch from the manual shaft.