For 1990-2009 cars

The driven member is a single clutch disc fitted with four torsional coil springs that are placed between the driven surface and the splined hub. These springs help reduce the shock of engine torque upon clutch engagement. The driven surface of the clutch disc consists of an asbestos material that is riveted onto the driven plate of the clutch disc and is resistant to frictional heat that can occur during clutch engagement and disengagement.