For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws (4) from the fuel filler door (2).
2. Remove the fuel filler door (2) from the vehicle.
3. Remove the retaining clip (3) and lock assembly (1) from the fuel filler door, if equipped.

### Installation Procedure

1. Install the lock assembly (1). Secure the lock assembly with the retaining clip.
2. Install the fuel filler door (2) to the vehicle. Secure the fuel filler door (2) with 2 screws (4).