For 1990-2009 cars

### Removal Procedure

1. Push in the head restraint release clips in order to pull the head restraint (1) out of the guide tubes (12).
2. Use a flat-bladed tool in order to gently pry the guide tubes (12) from the front seatback (11), by disengaging the retaining clips.

### Installation Procedure

1. Install the guide tubes (12) to the front seatback (11). Ensure that the retaining clips are fully engaged.
2. Push in the head restraint release clip in order to push the head restraint (1) into the guide tubes (12).