For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the light switch to the PARK position. | The following lamps are on:

• | All the parking lamps

• | The rear side marker lamps

• | The tail lamps

• | The license plate lamps

--

2 |

1. Turn the light switch to the OFF position.
2. Press the hazard switch to the ON position.

The following components flash approximately 80-90 times per minute:

• | The front turn lamps

• | The rear turn lamps

• | The left turn indicators

• | The right turn indicators

--

3 |

1. Press the hazard switch to the OFF position.
2. Depress the brake pedal.

The stoplamps illuminate.

--

4 | Release the brake pedal. | The stoplamps go out. | --
5 |

1. Turn the ignition switch to the ON position.
2. Press the turn signal switch to the left turn position.

The following components flash approximately 80-90 times per minute:

• | The left front turn lamps

• | The left rear turn lamps

• | The left turn indicator

--

6 | Press the turn signal switch to the right turn position. | The following components flash approximately 80-90 times per minute:

• | The right front turn lamps

• | The right rear turn lamps

• | The right turn indicator

--

7 | Press the turn signal switch to the OFF position. | The turn signal lamps stop flashing. | --
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.