For 1990-2009 cars

#### Tools required

• | J 34839 Pinion Bearing Remover

• | J 37764 Input Shaft Bearing Remover Adapter

• | J 23907 Slide Hammer with Bearing Adapter

• | J 7079-2 Universal Driver Handle Non-Threaded

• | J 34848 Clutch Pilot Bearing Installer

### Removal Procedure

1. Remove the manual transmission assembly from the vehicle. Refer to Two-Wheel-Drive Transmission Replacement or Four-Wheel-Drive Transmission Replacement in Manual Transmission.
2. Remove the pressure plate and the clutch disc from the flywheel. Refer to Clutch Assembly Replacement .
3. Remove the clutch pilot bearing (1) from the crankshaft using the J 37764 , J 34839 and the J 23907 .
4. Inspect the clutch pilot bearing (1) for scoring, binding or rough operation.
5. Replace as necessary.

### Installation Procedure

1. Install the clutch bearing into the crankshaft using the J 34848 with the J 7079-2 .
2. Install the clutch disc and the pressure plate to the flywheel (1). Refer to Clutch Assembly Replacement .
3. Install the manual transmission assembly into the vehicle. Refer to Two-Wheel-Drive Transmission Replacement or Four-Wheel-Drive Transmission Replacement in Manual Transmission.