For 1990-2009 cars

### Removal Procedure

1. Disconnect the 2 vacuum hoses (1) from the evaporative emission (EVAP) tank pressure control valve (5).
2. Disconnect the electrical connector (6) from the EVAP tank pressure control valve.
3. Remove the mounting bracket nut (2) retaining the EVAP tank pressure control valve .
4. Remove the EVAP tank pressure control valve from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the EVAP tank pressure control valve (5) to the vehicle with the nut (2).

Tighten
Tighten the nut to 1.6 N·m (14 lb in).

2. Connect the electrical connector (6) to the EVAP tank pressure control valve .
3. Connect the 2 vacuum hoses (1) to the EVAP tank pressure control valve (5).