For 1990-2009 cars

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 37979 Valve Spring Compressor Adaptor

• | J 38232 Valve Guide Seal Installer

1. Install the spring seat to the cylinder head.
2. Install the new valve seals using the J 38232 . Fully seat the seals on the valve guides.
3. Apply engine oil to the valve stem. Install the valve.

Important: Both the inner and outer valve springs have a top, large-pitch, and bottom, small pitch end. Install the small-pitch end toward the valve spring seat.

4. Install the springs.
5. Install the retainer.

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Compressed valve springs have high tension against the valve spring compressor. Valve springs that are not properly compressed by or released from the valve spring compressor can be ejected from the valve spring compressor with intense force. Use care when compressing or releasing the valve spring with the valve spring compressor and when removing or installing the valve stem keys. Failing to use care may cause personal injury.

6. Compress the valve spring using the J 8062 and the J 37979 .
7. Install the valve keepers.
8. Slowly release the J 8062 from the valve/spring assembly.
9. Lightly tap the valve stem tip with a plastic faced hammer and inspect for proper valve keeper seating.