For 1990-2009 cars

### Removal Procedure

1. Remove the front side door water deflector. Refer to Front Side Door Water Deflector Replacement .
2. Remove the front side door check pin (2) which secures the front side door check (3) to door jamb.
3. Remove the following components from the door:

• | The 2 bolts (1)

• | The door check (3)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the front side door check (3) to the door through the inner door panel access hole. Secure the check with the 2 bolts (1).

Tighten
Tighten the front side door check bolts to 10 N·m (89 lb in).

2. Install the door check (3) to the door jamb. Secure the check with the pin (2).
3. Install the front side door water deflector. Refer to Front Side Door Water Deflector Replacement .