For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
4-Speed Automatic Transmission (RPO M41)

- Bottom Pan Removal-2WD

2.8 L

3.0 qts

- Bottom Pan Removal-4WD

2.5 L

2.6 qts

- Complete Overhaul-2WD - 1.6L

7.2 L

7.6 qts

- Complete Overhaul-2WD - 2.0L

7.4 L

7.8 qts

- Complete Overhaul-2WD - 2.5L

7.4 L

7.8 qts

- Complete Overhaul -4WD - 1.6L

6.9 L

7.3 qts

- Complete Overhaul-4WD - 2.0L

7.1 L

7.5 qts

- Complete Overhaul-4WD - 2.5L

7.1 L

7.5 qts

5-Speed Manual Transmission (RPO M59)

- Two-Wheel-Drive Models

1.9 L

2.0 qts

- Four-Wheel-Drive Models

1.5 L

1.6 qts

Axle Housing

- Front

1.0 L

1.1 qts

- Rear

2.2 L

2.3 qts

Cooling System Capacity

- 1.6L Engine

5.5 L

5.8 qts

- 2.0L Engine

6.5 L

6.9 qts

- 2.5L Engine

8.0 L

8.5 qts

Engine Crankcase

- Without Filter Change 1.6L Engine

4.0 L

4.2 qts

- Without Filter Change 2.0L Engine

5.0 L

5.3 qts

- Without Filter Change 2.5L Engine

5.0 L

5.3 qts

- With Filter Change 1.6L Engine

4.2 L

4.4 qts

- With Filter Change 2.0L Engine

5.2 L

5.5 qts

- With Filter Change 2.5L Engine

5.5 L

5.8 qts

Fuel Tank

- 2-Door Convertible Models

56.0 L

14.8 gallons

- 4-Door Hardtop Models

66.0 L

17.4 gallons

Transfer Case 4WD Only | 1.7 L | 1.8 qts