For 1990-2009 cars

### Removal Procedure

1. Gently pry the rear end of the rear side marker lamp from the body in order to disengage the retaining clip.
2. Remove the rear side marker lamp bulb socket (1) from the rear side marker lamp (2).
3. Remove the bulb from the socket, as needed.

### Installation Procedure

1. Install the bulb to the socket, if removed.
2. Install the rear side marker lamp bulb socket (1) to the rear side marker lamp (2).
3. Install the rear side marker lamp to the vehicle.
4. Gently push the rear side marker lamp securely against the body in order to engage the retaining clip.